
Digital Repository Universitas Jember

**MAKALAH ILMIAH**

**PROSIDING SEMINAR INTERNASIONAL TERINDEKS SCOPUS**

**The 4th International Conference on Informatics and Computational Sciences (ICICoS)** 

****

Judul:

Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM

disusun oleh:

Sutikno, Khairul Anam, Azmi Saleh

**JURUSAN TEKNIK ELEKTRO**


**FAKULTAS TEKNIK**


**UNIVERSITAS JEMBER**

**2021**

Diseminarkan Secara Virtual

10 - 11 November 2020

Digital Repository Universitas Jember

**ICICoS 2020** 

**10 - 11 November 2020**

**Proceeding**

**The 4th International Conference**

**on Informatics and Computational Sciences**

**Organized by:**

Department of Informatics

Faculty of Science and Mathematics Universitas Diponegoro

**Sponsored by:**


**Part Number : CFP20N15-ART**

**ISBN : 978-1-7281-9526-1**

Digital Repository Universitas Jember

**COPY RIGHT**

**2020 4th International Conference on Informatics and Computational Sciences (ICICoS) took place November 10-11, 2020**

Copyright and Reprint Permission: Abstracting is permitted with credit to the source. Libraries are permitted to photocopy beyond the limit of U.S. copyright law for private use of patrons those articles in this volume that carry a code at the bottom of the first page, provided the per-copy fee indicated in the code is paid through Copyright Clearance Center, 222 Rosewood Drive, Danvers, MA 01923. 

For other copying, reprint or republication permission, write to IEEE Copyrights Manager, IEEE Operations Center, 445 Hoes Lane, Piscataway, NJ 08854.

All rights reserved. Copyright © 2020 by IEEE.

**ISBN: 978-1-7281-9526-1**

**IEEE catalog number: CFP20N15-ART**


Digital Repository Universitas Jember

**WELCOME SPEECH FROM THE GENERAL CHAIR OF ICICoS 2020**

On behalf of the organizing committee, I am delighted to welcome all 

participants to the 4th International Conference on Informatics and

Computational Sciences (ICICoS 2020). This conference is the fourth

international conference held by Department of Informatics, 

Universitas Diponegoro in Semarang from November 10th to

November 11th, 2020.

In this conference, the committee decided to choose the following

theme: “Accelerating Informatics and Computational Research for

Society 5.0”. This topic is in line with the concept of Society 5.0 which

was introduced by Japan and inaugurated on January 21, 2019.

Society 5.0 is a human-centered society that balances economic

advancement with the resolution of social problems by a system that highly integrates cyberspace and physical space. This concept was born as a development of the 4.0 industrial revolution which is considered to degrade the role of humans. The aim of the conference is to provide an interactive international forum for sharing and exchanging information on the latest research in the area of computer sciences, informatics, computational science, and related field, which contribute to the society 5.0.

Nearly 110 academicians, researcher, practitioner and presenters from 9 countries (Indonesia, United State of America, France, Austria, Australia, Japan, Timor Leste, Malaysia, and The Netherlands) have gathered in this event. In total, there are 84 active papers submitted to this conference. Each paper has been reviewed with tight criteria from our invited reviewers. Based on the review result, papers have been accepted, which lead to an acceptance rate of 47.6%.

This conference will not be successful without extensive effort from many parties. First, I would like to thank all keynote speakers for allocating their valuable time to share their knowledge with us. I would also like to express my sincere gratitude to all participants who participate in this conference. Special acknowledgement should go to the Technical Program Committee Chairs, Members, and Reviewers for their thorough and timely reviewing of the papers. We would also like to thank our sponsors: IEEE Indonesia Section and Research and Society Service Institution Universitas Diponegoro, who have helped us to keep down the costs of ICICoS 2020 for all participants. Last but not least, recognition should also go to the Local Organizing Committee members who have put enormous effort and support for this conference.

At last, we hope that you have an enjoyable and inspiring moment during our conference. Thank you for your participation on ICICoS 2020.

Dr. Dinar Mutiara Kusumo Nugraheni, ST, M Info Tech(Comp)

General Chair of ICICoS 2020

Digital Repository Universitas Jember


**COMMITTEES**

**Steering Committee:**

• Prof. Widowati, Universitas Diponegoro, ID

• Prof. W. Jatmiko, Universitas Indonesia, ID

• Prof. J. Jamari, Universitas Diponegoro, ID

• R. Kusumaningrum, Universitas Diponegoro, ID 

• Kurnianingsih, Politeknik Negeri Semarang, ID

• NA. Setiawan, Universitas

**General Chair:**

• DMK. Nugraheni, Universitas Diponegoro, ID

**General Co-chairs:**

• PW. Wirawan, Universitas Diponegoro, ID

• R. Saputra, Universitas Diponegoro, ID

**Secretary:**

• S. Adhy, Universitas Diponegoro, ID

• SN. Endah, Universitas Diponegoro, ID

**Finance:**

• B. Noranita, Universitas Diponegoro, ID

• Khadijah, Universitas Diponegoro, ID

**Program Chair:**

• FA. Nugroho, Universitas Diponegoro, ID

**Publication Chair:**

• Rismiyati, Universitas Diponegoro, ID

• E. Suharto, Universitas Diponegoro, ID

**Technical Program Committee Chairs:**

• A. Wibowo, Universitas Diponegoro, ID

• MA. Riyadi, Universitas Diponegoro, ID

**Technical Program Committee Member:**

• AH. Ali, Universiti Kuala Lumpur, MY

• A. Alsobeh, Yarmouk University, JOR

• A. Antonyova, University of Prešov in Prešov, SVK

• A. Azizan, Universiti Teknologi Malaysia (UTM), MY

• A. Bagwari, IEEE Member, UTU, IN

• A. Ghasempour, ICT Faculty, USA

• A. Hamad, University of Baghdad, IRQ

Digital Repository Universitas Jember

• A. Miry, Al-Mustansiriyah University, IRQ

• A. Mobashsher, The University of Queensland, AU


• AM. Nasrabadi, Shahed University, IRN

• A. Mukherjee, Jiangsu University, CN

• A. Najmurrokhman, Universitas Jenderal Achmad Yani, ID

• AP. Widodo, Diponegoro University, ID

• A. Rafiei, University of Technology Sydney, AU

• A. Sallam, Taiz University, YEM 

• A. Sharma, Quantum University, Roorkee, Uttarakhand, IND

• AS. Shibghatullah, UCSI University, MY

• A. Sunyoto, Universitas Amikom Yogyakarta, ID

• A. Testa Ministry of Economy and Finance, ITA

• A. Wibowo, Diponegoro University, ID

• B. Jiang, The City University of New York, USA

• B. Warsito, Diponegoro University, ID

• C. Kerdvibulvech, National Institute of Development Administration, THA • C. Sonagiri, Institute of Aeronautical Engineering, IND

• C. Yuen, Singapore University of Technology and Design, SG

• D. Andriana, Indonesian Institute of Sciences, ID

• D. Chisanga, The University of Zambia, ZMB

• D. Ciuonzo, University of Naples Federico II, ITA

• DH. Fudholi, Universitas Islam Indonesia, ID

• D. Krstić, Faculty of Electronic Engineering, University of Niš, SRB

• DMK. Nugraheni, Universitas Diponegoro, ID

• D. Nurjanah, Telkom University, ID

• D. Wijaya, Telkom University, ID

• E. Babulak, Liberty University, USA

• E. Jiménez Macías, University of La Rioja, ESP

• E. Kaburuan, BINUS University, ID

• E. Werbin, Universidad Nacional de Cordoba, ARG

• F. Aadil, COMSATS University Islamabad Attock Campus, PAK

• F. Farikin, Diponegoro University, ID

• G. Abbas, GIK Institute of Engineering Sciences & Technology, PAK

• G. Dekoulis, Aerospace Engineering Institute (AEI), CYP

• G. Palmerini, Sapienza Università di Roma, ITA

• G. Tambouratzis, Institute for Language & Speech Processing, GRC

• H. Abdulkareem, Al-Nahrain University, IRQ

• H. Alasadi, IRAQ- BASRA, IRQ

• H. El Abed, Technical Trainers College (TTC), SA

• H. Khattak, COMSATS University, Islamabad, PAK

• H. Ng, Multimedia University, MY

• H. Pan, New Jersey Institute of Technology, USA

• H. Pardede, Indonesian Institute of Sciences, ID

• HLH. Spits Warnars, Bina Nusantara University, ID

• H. Toba, Maranatha Christian University, ID

Digital Repository Universitas Jember

• I. Song, Korea Advanced Institute of Science and Technology, KOR

• I. Yulita, Universitas Padjadjaran, ID


• J. Ali, University of Technology, IRQ

• J. Chin, Multimedia University, MY

• J. Suba, University of the Assumption, PHL

• K. Al-Saedi, Mustansiriyah University, IRQ

• K. Hopkinson, Air Force Institute of Technology, USA

• K. Kabassi, Ionian University, GRC 

• K. Majumder, West Bengal University of Technology, IND

• L. Boubchir, University of Paris 8, FR

• MA. Ahmad, Universiti Malaysia Pahang, MY

• MKI. Ahmad, Universiti Tun Hussein Onn Malaysia, my

• M. Chen, Electrical Engineering, Da-Yeh University, TW

• M. Hasibuan, University Gadjah Mada, ID

• M. Koyimatu, Universitas Pertamina, ID

• M. Mustaffa, Universiti Putra Malaysia, MY

• M. Nyirenda, University of Zambia, ZM

• M. Riasetiawan, Universitas Gadjah Mada, ID

• M. Riyadi, Diponegoro University, ID

• M. Tuloli, Universitas Negeri Gorontalo, ID

• M. Younis, University of Baghdad, IRQ

• M. Yusuf, University of Trunojoyo, ID

• N. Al-Azzawi, Baghdad University, IRQ

• NC. Basjaruddin, Politeknik Negeri Bandung, ID

• N. Che Pa, Universiti Putra Malaysia, MY

• N. Ifada, University of Trunojoyo Madura, ID

• N. Ojha, Sharda University, Greater Noida, UP, IND

• N. Prabaharan, SASTRA Deemed University, IND

• O. Ridha , University of Baghdad, IRQ

• O. Manad, UMANIS SA, FR

• P. Corral, Miguel Hernández University, ES

• P. Crippa, Università Politecnica delle Marche, ITA

• P. Mursanto, Universitas Indonesia, ID

• P. Zhang, Stony Brook University, USA

• R. Agustin, Universitas Pasundan, ID

• R. Fyath, Al-Nahrain University, College of Engineering, IRQ

• RC. Herrera Lara, National Polytechnic School, EC

• R. Kusumaningrum, Diponegoro University, ID

• R. Ngadiran, Universiti Malaysia Perlis, MY

• R. Nugroho, Soegijapranata Catholic University, AU

• R. Palma-Orozco, Instituto Politécnico Nacional, MX

• S. Alkassar, Ninevah University, IRQ

• S. Birla, Manipal University Jaipur, IND

• S. Biryuchinskiy, Vigitek, Inc, USA

• S. Horng , National Taiwan University of Science and Technology, TW

Digital Repository Universitas Jember

• S. Mardiyanto, Institut Teknologi Bandung, ID

• S. Nazir, University of Peshawar, PAK

• S. Ooi, Multimedia University, MY

• S. Sarkar, Vijaya Vittala Institute of Technology, IND

• S. Singh, Manipal Institute of Technology, IND

• S. Suryono, Diponegoro University, ID

• S. Tadisetty, Kakatiya University College of Engineering and Technology, IND • S. Tan, Newcastle University, GB 

• T. Chen, MAXEDA Technology, TW

• T. Manjunath, Dayananda Sagar College of Engineering, Bangalore, Karnataka, IND • T. Nguyen, Purdue University Fort Wayne, USA

• T. Yingthawornsuk, King Mongkut's University of Technology Thonburi, THA • V. Ramos, Universidad Autonoma Metropolitana, MX

• V. Omwenga, Strathmore University, KEN

• W. Sunindyo, Institut Teknologi Bandung, ID

• W. Suwarningsih, Indonesian Institute of Science, ID

• Y. Su, Shu-Te University, TW

• Z. Mekkioui, University of tlemcen, DZ

Digital Repository Universitas Jember

**PROGRAM SCHEDULE**

**Tuesday, November 10th, 2020**

| **Time** | **Event** | **Event Details** | | | |
| --- | --- | --- | --- | --- | --- |
| 08.00 - 08.30 | Participants entering virtual conference room | | | | |
| 08.30 - 08.35 | Opening  Ceremony | Welcome Speech from the General Chair of ICICoS 2020 **(Dr. Dinar Mutiara KN, M. Info. Tech)** | | | |
| 08.35 - 08.40 | Welcome Speech from IEEE IS | | | |
| 08.40 - 08.50 | Welcome Speech from the Dean of Faculty of Science and Mathematics, Universitas Diponegoro  **(Prof. Dr. Widowati, M.Si)** | | | |
| 08.50 - 09.00 | Opening Speech from the Rector Universitas Diponegoro **(Prof. Dr. Yos Johan Utama, S.H., M.Hum.)** | | | |
| 09.00 – 10.30 | Plenary I | • Keynote Speaker I:  **Assoc Prof. AbdulRahman A. AlSewari**  • Moderator:  **Edy Suharto, ST, M.Kom** | | | |
| 10.30 – 12.00 | Plenary II | • Keynote Speaker II:  **Dr. Eng. Sunu Wibirama, S.T., M.Eng**.  • Moderator:  **Fajar Nugroho, S.Kom, M.Cs** | | | |
| 12.00 - 13.00 | Break | | | | |
| 13.00 – 1**4.3**0 | Parallel Session I | | | | |
| Room 1  Information System | | Room 2  Software  Engineering,  Network and  Data Mining | Room 3  Machine Learning and It’s  Applications 1 | Room 4  Machine Learning and It’s  Applications 2 |
| **14.30 - 15.00** | Break | | | | |

Digital Repository Universitas Jember



| **15.00 – 16.15** | Parallel Session II | | | |
| --- | --- | --- | --- | --- |
| Room 1  Information System | Room 2  Software  Engineering,  Network and  Data Mining | Room 3  Machine Learning and It’s  Applications 1 | Room 4  Machine Learning and It’s  Applications 2 |
| 1**6**.**15** – 16.3**0** | Closing Ceremony | | | |

**Wednesday, November 11th, 2020** 

• Workshop

Digital Repository Universitas Jember



**PROGRAM SCHEDULE – Parallel Session Schedule**

| **Parallel Session – Room 1**  **Information System** | | | | |
| --- | --- | --- | --- | --- |
| **Session** | **Time** | **Paper ID** | **Author** | **Title** |
| **1**  **n**  **o**  **i**  **s**  **s**  **e**  **S**  **l**  **e**  **l**  **l**  **a**  **r**  **a**  **P** | 13.00  –  13.15 | 1570657493 | Meyliana Meyliana, Henry Widjaja, Stephen Santoso, Surjandy Surjandy, Erick  Fernando, Andreas Raharto Condrobimo | Improving the Quality of Learning Management System (LMS) based on Student Perspectives Using UTAUT2 and Trust Model |
| 13.15  –  13.30 | 1570660660 | Aulia-Absari Khalil, Meyliana, Achmad Nizar Hidayanto, Harjanto Prabowo | Identification of Factor Affecting Continuance Usage Intention of mHealth Application |
| 13.30  –  13.45 | 1570669017 | Julius Galih Prima Negara, Djoko Budiyanto Setyohadi, Pranowo | Uncertainty Avoidance and  Individualism Collectivism on Acceptance of Smart City Mobile Applications |
| 13.45  –  14.00 | 1570670167 | Zerlita Fahdha Pusdiktasari, Rahma Fitriani, Eni  Sumarminingsih | The Outlierness Degree of Spatial Observations in the Presence of Spatial Outliers, Simulation Study using Average Difference Algorithm |
| 14.00  –  14.15 | 1570670570 | Ragil Saputra, Tusta Rayana, Satriyo Adhy, Nurdin Bahtiar, Melnyi Timu | Success Factor Affecting M  Learning Implementation:  Perspective of Students |
| 14.15  –  14.30 | 1570671361 | Aang Kisnu Darmawan, Daniel Siahaan, Tony Dwi Susanto, Hoiriyah Hoiriyah, Busro Umam Achmad Nizar  Hidayanto, A'ang Subiyakto, Miftahul Walid, Iwan Santosa | Hien's Framework for Examining Information System Quality of Mobile-based Smart Regency Service in Madura Island Districts |
|  | 14.30  –  15.00 | COFFEE BREAK | | |
| **2**  **n**  **o**  **i**  **s**  **s**  **e**  **S**  **l**  **e**  **l**  **l**  **a**  **r**  **a**  **P** | 15.00  –  15.15 | 1570674375 | Dinar Mutiara Kusumo  Nugraheni, Amabel  Hadisoewono, Beta Noranita | Continuance Intention to Use (CIU) on Technology Acceptance Model (TAM) for m-payment (case study: TIX ID) |
| 15.15  –  15.30 | 1570677311 | Ragil Saputra, Satriyo Adhy, Nurdin Bahtiar, Nauli Isnaini, Zaenal Abidin, Edy Suharto | Factors Influencing Student's Adoption of E-Learning in  Indonesian Secondary Schools |
| 15.30  –  15.45 | 1570677382 | Indra Waspada, Riyanarto Sarno | An Improved Method of Graph Edit Distance for Business Process Model Similarity Measurement |

Digital Repository Universitas Jember



| **Parallel Session – Room 4**  **Machine Learning and Its Applications 2** | | | | |
| --- | --- | --- | --- | --- |
| **Session** | **Time** | **Paper ID** | **Author** | **Title** |
| **1**  **n**  **o**  **i**  **s**  **s**  **e**  **S**  **l**  **e**  **l**  **l**  **a**  **r**  **a**  **P** | 13.00  –  13.15 | 1570666720 | Cuk Tho, Harco Leslie Hendric Spits Warnars, Benfano Soewito, Ford Lumban Gaol | Code-mixed Sentiment Analysis using Machine Learning Approach - A Systematic Literature Review |
| 13.15  –  13.30 | 1570670508 | Muhammad Rizky Ramadhan, Sukmawati Nur Endah,  Aprinaldi Bin Jasa Mantau | Implementation of Textrank  Algorithm in Product Review Summarization |
| 13.30  –  13.45 | 1570674565 | Moh Abdul Latief, Alhadi Bustamam, Titin Siswantining | Performance Evaluation XGBoost in Handling Missing Value on  Classification of Hepatocellular Carcinoma Gene Expression Data |
| 13.45  –  14.00 | 1570674664 | Ika Marta Sari, Saskya  Soemartojo, Titin Siswantining, Devvi Sarwinda | Mining Biological Information from 3D Medulloblastoma Cancerous Gene Expression Data Using  TimesVector Triclustering Method |
| 14.00  –  14.15 | 1570674674 | Dea Siska, Titin Siswantining, Devvi Sarwinda, Saskya  Soemartojo | Triclustering Algorithm for 3D Gene Expression Data Analysis using Order Preserving Triclustering (OPTricluster) |
| 14.15  –  14.30 | 1570676322 | Agung Wiratmo, Chastine Fatichah | Assessment of Indonesian Short Essay using Transfer Learning Siamese Dependency Tree-LSTM |
|  | 14.30  –  15.00 | COFFEE BREAK | | |
| **2**  **n**  **o**  **i**  **s**  **s**  **e**  **S**  **l**  **e**  **l**  **l**  **a**  **r**  **a**  **P** | 15.00  –  15.15 | 1570676889 | Sayyidah Hanifah Putri, Adhi Harmoko Saputro | Design of Convolutional Neural Network Modeling for Low-Density Lipoprotein (LDL) Levels  Measurement Based on Iridology |
| 15.15  –  15.30 | 1570676890 | Dyla Velia, Adhi Harmoko Saputro | Designing Diabetes Mellitus  Detection System Based on  Iridology with Convolutional Neural Network Modeling |
| 15.30  –  15.45 | 1570677039 | Rismiyati, Sukmawati Nur Endah, Khadijah, Ilman Nabil Shiddiq | Xception Architecture Transfer Learning for Garbage Classification |
| 15.45  –  16.00 | 1570677362 | Sutikno Sutikno, Khairul Anam, Azmi Saleh | Voice controlled wheelchair for disabled patients based on CNN & LSTM |

24/2/2021 Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM - IEEE Conference Publication

Digital Repository Universitas Jember Personal Sign In IEEE.org IEEE *Xplore* IEEE-SA IEEE Spectrum More Sites **SUBSCRIBE SUBSCRIBE**Cart Create Account

 Browse  My Settings  Help  Institutional Sign In Institutional Sign In

**All** 

Conferences > 2020 4th International Confer... 

**Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM**

**Publisher: IEEE Cite This Cite This**  **PDF**

<< Results

Sutikno ; Khairul Anam ; Azmi Saleh **All Authors**



**ADVANCED SEARCH**  Back to Results

**5**

Full

Text Views

**Abstract**

Document Sections I. Introduction

Downl PDF

 

**Alerts**

Manage

Content Alerts

Add to Citation

Alerts

Export to

Collabratec

**More Like This**

Speech recognition based robotic system of wheelchair for disable people

2016 International Conference on Communication and Electronics Systems (ICCES)

Published: 2016

Smart Wheelchair to Facilitate Disabled Individuals

2019 International Conference on Advancements in Computing (ICAC) Published: 2019

**Show More**

II. Proposed Method

III. Results and Discussion

 Conclusion

Authors

Figures

References

Keywords

Metrics

More Like This

**Abstract:**Disabled patients with reduced mobility due to health problems such as disability, injury, paralysis, or other factors will experience difficulty in movement. They need t... **View more**

**Metadata**

**Abstract:**

Disabled patients with reduced mobility due to health problems such as disability, injury, paralysis, or other factors will experience difficulty in movement. They need tools that can help them, in which the most widely used is a wheelchair. The main objective of this research is to control wheelchair motion with voice commands. There are five commands for wheelchair control: forward, backward, right, left, and stop. Voice data is obtained from recording several subjects using Sound Recorder Pro and Sox Sound Exchange. The voice commands for wheelchair navigation were identified using Convolutional Neural Network (CNN) and Long Short-Term Memory (LSTM) combination embedded in Raspberry Pi 3. Voice data is first converted to spectrogram images before being fed into CNN using Mel-Frequency Cepstrum Coefficients (MFCC). This system can be controlled by simple voice commands given by the user. This method is proven to be useful in speech recognition with an accuracy level using CNN LSTM above 97.80 %. Preliminary experimental results indicate that voice commands in wheelchairs using the CNN-LSTM can be recognized well.

https://ieeexplore.ieee.org/document/9299007 1/3

24/2/2021 Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM - IEEE Conference Publication

Digital Repository Universitas Jember**Published in:** 2020 4th International Conference on Informatics and Computational Sciences (ICICoS)

**Date of Conference:** 10-11 Nov. 2020

**INSPEC Accession Number:** 20304257

**Date Added to IEEE *Xplore*:** 24 December

**DOI:** 10.1109/ICICoS51170.2020.9299007

2020

**ISBN Information: I. Introduction**

**Publisher:** IEEE

**Conference Location:** Semarang, Indonesia

 **Contents**

Persons with disabilities have many inconveniences in their lives. The disability that they suffer from can be physical, mental, intellectual, or even sensory. These difficulties can limit them to fully and effectively participate in society [1] . According to a survey conducted by the World Health Organization (WHO), it estimated that more than 1 billion people 

Sign in to Continue Reading

in the world have a disability in some form of disability [2] . Meanwhile, the 2010 PUSDATIN data from the Ministry of Social Affairs in

Indonesia, was 11,580,117 in which 3,010,380 of them were physically impaired [3] .

**Authors**  **Figures**  **References**  **Keywords**  **Metrics** 

**IEEE Personal Account** CHANGE USERNAME/PASSWORD

**Purchase Details**

PAYMENT OPTIONS

VIEW PURCHASED DOCUMENTS

**Profile Information**

COMMUNICATIONS PREFERENCES PROFESSION AND EDUCATION TECHNICAL INTERESTS

**Need Help?**

US & CANADA: +1 800 678 4333 WORLDWIDE: +1 732 981 0060 CONTACT & SUPPORT

**Follow**

  

About IEEE *Xplore* | Contact Us | Help | Accessibility | Terms of Use | Nondiscrimination Policy | Sitemap | Privacy & Opting Out of Cookies A not-for-profit organization, IEEE is the world's largest technical professional organization dedicated to advancing technology for the benefit of humanity.

© Copyright 2021 IEEE - All rights reserved. Use of this web site signifies your agreement to the terms and conditions.

**IEEE Account**

» Change Username/Password » Update Address

**Purchase Details**

»Payment Options

»Order History

»View Purchased Documents

**Profile Information**

» Communications Preferences »Profession and Education »Technical Interests

**Need Help?**

» **US & Canada:** +1 800 678 4333 »**Worldwide:** +1 732 981 0060 » Contact & Support

https://ieeexplore.ieee.org/document/9299007 2/3

24/2/2021 Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM - IEEE Conference Publication About IEEE *Xplore* | Contact Us | HelpDigital Repository Universitas Jember | Accessibility | Terms of Use | Nondiscrimination Policy | Sitemap | Privacy & Opting Out of Cookies

A not-for-profit organization, IEEE is the world's largest technical professional organization dedicated to advancing technology for the benefit of humanity. © Copyright 2021 IEEE - All rights reserved. Use of this web site signifies your agreement to the terms and conditions.

https://ieeexplore.ieee.org/document/9299007 3/3

2020 4th International Conference on Informatics and Computational Sciences (ICICoS)

Digital Repository Universitas Jember

Voice Controlled Wheelchair for Disabled Patients based on CNN and LSTM

Sutikno

*Dept. of Electrical Engineering University of Jember*

Jember, Indonesia

email: sutikno@unmuhjember.ac.id

Khairul Anam

*Dept. of Electrical Engineering University of Jember*

Jember, Indonesia

email: khairul@unej.ac.id

Azmi Saleh

*Dept. of Electrical Engineering University of Jember*

Jember, Indonesia

email: azmi2009@gmail.com

***Abstract*—Disabled patients with reduced mobility due to health problems such as disability, injury, paralysis, or other factors will experience difficulty in movement. They need tools that can help them, in which the most widely used is a wheelchair. The main objective of this research is to control wheelchair motion with voice commands. There are five commands for wheelchair control: forward, backward, right, left, and stop. Voice data is obtained from recording several subjects using Sound Recorder Pro and Sox Sound Exchange. The voice commands for wheelchair navigation were identified using Convolutional Neural Network (CNN) and Long Short Term Memory (LSTM) combination embedded in Raspberry Pi 3. Voice data is first converted to spectrogram images before being fed into CNN using Mel-Frequency Cepstrum Coefficients (MFCC). This system can be controlled by simple voice commands given by the user. This method is proven to be useful in speech recognition with an accuracy level using CNN-LSTM above 97.80 %. Preliminary experimental results indicate that voice commands in wheelchairs using the CNN-LSTM can be recognized well.**

***Keywords—disability, wheelchair, MFCC, CNN, LSTM***

I. INTRODUCTION

Persons with disabilities have many inconveniences in their lives. The disability that they suffer from can be physical, mental, intellectual, or even sensory. These difficulties can limit them to fully and effectively participate in society [1]. According to a survey conducted by the World Health Organization (WHO), it estimated that more than 1 billion people in the world have a disability in some form of disability [2]. Meanwhile, the 2010 PUSDATIN data from the Ministry of Social Affairs in Indonesia, was 11,580,117 in which 3,010,380 of them were physically impaired [3].

In the biomedical sector, wheelchairs are a vital device because of the latest advancements in the industrial population. Demand for patients with particular limitations is increasing because intelligent wheelchairs will play an essential role in the welfare society in the future. The use of intelligent wheelchairs inspires machines' view as partners and not as instruments [4]. In previous studies, many articles discussed introducing voice commands for wheelchair navigation in prototype form, using Arduino, ANN, Fuzzy, and other intelligence microcontrollers [5] [6]. Nevertheless, only a few use comparisons between the Convolutional Neural Network (CNN) and Long short-term memory (LSTM) methods for speech recognition applied to wheelchairs. Besides, the prior study's main objective of this wheelchair system is the addition of electric wheelchairs using sound

978-1-7281-9526-1/20/$31.00 ©2020 IEEE

conversion technology to drive electric wheelchairs using the CNN-LSTM network embedded in Raspberry Pi 3.

In the future, this smart wheelchair will have a significant impact on the disabled. As a result, electric wheelchairs that use speech identification technology can help to direct wheelchairs and plan movements in a better way to facilitate patient life. The speech recognition system is used as a user interface in operating the system in the system presented. Patients who are categorically unable to walk and must use a wheelchair for their daily work can control the wheelchair's movement only with their voice commands. When using this wheelchair, people will be able to move more independently. The wheelchair control uses speech recognition to trigger and control all movements [7]. The main emphasis is undoubtedly to concentrate on improving the wheelchair by incorporating several new features as its advantages [8]. 

II. PROPOSED METHOD

In general, the block diagram is a general description of the system to be built. It is necessary to make a block diagram/process flow that can help the readers to understand the research's flow and process quickly. Fig. 1 indicates the process flow of this study.

*A. Preparation of the dataset*

The sound recording process was carried out to obtain a dataset. The recording used a Sound Recorder Pro application and Sound Meter as a tool to detect the ambient noise level. Some parameters and variables were recorded, as shown in table 1.

Fig. 1. The proposed block diagram

2020 4th International Conference on Informatics and Computational Sciences (ICICoS) Digital Repository Universitas Jember

TABLE I. VOICE RECORDING PARAMETERS

| ***Variabel*** | ***Information*** |
| --- | --- |
| Data type | Sound (forward, backward, left, right, stop). |
| Sample rate, bitrate | 16.000 Hz, 128 Kbit/s |
| The duration of each word | 1 – 2 second. |
| Storage Format | \*.wav (PCM) |
| Channels, sources | Mono/stereo/ microphone |
| Number of sound samples | 1000 / word |
| Recording time | Adjusted |
| Recording location | Space is closed and open |



Fig. 2. Illustration of the trim and the pad process

In the table above, the recorded voice commands are

popular method in varied applications, which need voice preprocessing before being implemented. In its running process, MFCC works based on the difference in frequency of the human ear. Therefore, it can indicate the real human sound signals. Usually, the sampling frequency used is above 10.000 Hz to minimize the aliasing effect of the analog digital conversion. The following Fig. 3 is how the MFCC process works.

The input form of voice data is in the .wav with a 16,000 Hz sample as test data and training data. Frame blocking is a condition where a signal is segmented into overlapping frames. Windowing aims to minimize signal friction of each frame starting from the beginning to the end. If the window is defined as w(n), 0 ≤ n ≤ N-1, where N is the number of samples in each frame, the result of signal windowing is:

*Y1*(*n*)*= x1*(*n*) *w*(*n*)*, 0 ≤ n ≤ N-1* (1) *w*(*n*) *= 0.54 - 0.46 cos* (*2πn*

*N-1*) *, 0 ≤ n ≤ N-1* (2)

Where *w(n)* is the resulting window frames, *N* is the number of sample values per frame, and *n* is the number of frames. The next step is a Fast Fourier Transform (FFT), which is a fast algorithm for implementing a discrete Fourier transform (DFT). FFT can change each sample N frame from the time to frequency domain, which is formulated bellow:

*k=0 eps* (*-2πjkn*

*N-1*

forward, backward, right, left, and stop using a microphone

*Xn =* ∑ *xk*

*N*) *, n = 0,1,2,……N-1* (3)

with a sample rate of 16.000 Hz, assisted by using a Sound Recorder Pro application recorded in .wav format. Each command was recorded as many as 1000. Meanwhile, the location recording was done in a closed and open space with a noise level of 33.0 - 83.8 decibels. After the data was recorded, the process went to the preprocessing stage to get the same size using the notepad and Sox-Sound Exchange tools. This stage aims to make the data uniform and easier to use as input to the system to be created. The command to do is trim forward 0.1 seconds, trim back 0.1 seconds, pad 2 seconds, and trim 1 second using Sox-Sound Exchange, as shown in Fig. 2. Trim is the process of cutting data from time 0 to time t, while pad adds silence to the sound until the sound reaches t. From this process, the voice data is ready to be a dataset. 

*B. Mel-Frequency Cepstrum Coefficients (MFCC) Method* The next step is visualized data. Since the data is a one dimensional vector, it makes the visualization process easier. However, it is necessary to know that the speech recognition process rarely uses raw data. Instead, it usually uses an approach of converting from an audio file into a spectrogram. The methods often used to analyze audio/voice signals are Mel-Frequency Cepstrum Coefficients (MFCC) and Short Time Fourier Transform (STFT) [9] [10]. In this study, the method employs MFCC to convert audio files into image spectrograms. The MFCC method is one of the domain methods and is most commonly used to perform feature extraction. MFCC is considered a frequency domain feature that is much more accurate than a time-domain feature for converting the voice signal into several parameters [11]. The reason why MFCC is chosen to be employed is the proof of its representation in signals. As a result, it becomes the most

Xn is the frequency, xk is the sample value, N is the number of sample data, and j is the imaginary number. The subsequent step is the Mel-Frequency Wrapping stage. The measurement used to get voice signal with actual frequency f is usually in Hz. A subjective pitch is measured on a scale of “Mel”. The scale of the Mel-frequency is a linear low frequency and a high logarithmic frequency, each consisting of under 1000 Hz and over 1000 Hz, respectively. This scale is defined as:

*Xi =log10* ( ∑ |*X*(*k*)|*Hi(k) N-1*

*k=0* )*, i=1,2,3…..,M* (4)

*Hi(k)* is the value of the filter triangle *I*, *X(k)* is the value of *k* data from the FFT process, *M* is the number of filters, and *N* is the number of data. The final step is to change the log mel spectrum into the time domain, which results in the Cepstrum Mel Frequency Coefficient (MFCC). Cepstrum is the opposite designation for a spectrum. Cepstrum is generally used to gather information from a voice signal spoken by humans. The log Mel spectrum as a final stage is changed to cepstrum using Discrete Cosine Transform (DCT). The following equations are used in the cosine transformation:

���� *=* ∑ *Xi* ������ M*i=0* (��(�� −1)/2����) (5)

*j* is 1,2,3,…. *K* (*K* is the number of coefficients intended and M is the number of filters). The results of the MFCC process for sound signals can be seen in Fig. 4.

2020 4th International Conference on Informatics and Computational Sciences (ICICoS) Digital Repository Universitas Jember

being parts of LSTM architecture. Each cell has three main 

components responsible for forgetting, remembering, and

updating data [15]. Fig. 6 shows how the LSTM architecture

is. Just like RNN, the LSTM also consists of modules with

processing. What makes it different is that the LSTM

modules are from themselves.

The LSTM decides any information needed to be

removed from the *Ct-1* cell, taking advantage of a sigmoid

Fig. 3. Block diagram of MFCC process [12].



Fig. 4. Spectrogram of forwards, backwards, right, left, stop commands. 

Fig. 5. Convolutional neural network architecture

*C. Convolutional Neural Network (CNN)*

The CNN method as a type of neural network is commonly used to proses any image data [13]. This method can detect any objects in the form of images, in which it is almost the same as ordinary neural networks. Its architecture comprises of neurons equipped with heavy, biased, and activated functions. Since CNN has more networks and it is widely applied to image data, it is usually categorized as Deep Neural Network. In its running process, there are two methods that have been categorized as feedforward and backpropagation. The way CNN works is similar to Multi Layer Perceptron (MLP), where each neuron has only one dimension. However, each CNN neuron is shown in a two

dimensional form, making it different from MLP. The CNN architecture in this study is shown in Fig. 5. The CNN architecture that was built consisted of inputs, Feature Learning Layers, Fully Connected Layer, and Output as Classification.

Input for CNN is in the form of a spectrogram image. A matrix represents this image with a size of 20 x 11. Layer 1, layer 2, and layer 3 are the convolutional layer. Convolutional layer 1 consists of 32 filter layers where the convolution happens between receptive fields and kernels of 3 x 3 using the same padding and stride 1. This architecture is also applied to layer 2 and layer 3. All receptive fields will be in the partial overlap. All neurons will share the weight of the connection [14].

*D. Long Short-Term memory (LSTM)*

The LSTM is a particular type of Recurrent Neural Network (RNN), capable of studying long-term and short term data. LSTM works through several cells, which are

gate called the “forget gate” *ft* . This gate is capable of reading the values *ht-1* and *xt* , and producing a number between 0 and 1 for each element in *Ct-1*. A value of 1 means “really take care of this element”, while 0 means “get rid of this element completely”. The following is the forget gate and the gates element-wise sum formula:

*ft= σ ( Wf.* [ *ht-1, xt*]*+ bf*(6) *it= σ ( Wi.* [ *ht-1, xt* ]*+ bi* (7) *Ĉt= tanh ( Wc.* [ *ht-1, xt* ]*+ bC* (8)

The last part of the LSTM is the output gate (neuron layer with the sigmoid activation function at the far right of the neuron layer line). This gate output does not contribute to the state of the cell, but it is this gate that differentiates the cell state and the actual output. The result of the LSTM can be seen in the following:

*ot= σ ( Wo.* [ *ht-1, xt* ]*+ b0* (9)

*ht= ot. tanh ( Ct)* (10)

The LSTM structure using voice commands is shown in Fig. 7.



Fig. 6. The architecture of the LSTM.



Fig. 7. LSTM architecture for speech recognition

2020 4th International Conference on Informatics and Computational Sciences (ICICoS)

Digital Repository Universitas Jember



Fig. 8. Architecture of CNN-LSTM 



Fig. 9. Wheelchair hardware and electric design

*E. CNN – LSTM Classifier*

A way to analyze audio/voice signals is a 2-dimensional representation, where time-frequency analysis is commonly used to process sound signals. In this study, the voice signal is converted into 2D representation using Mel Frequency Cepstrum Coefficient (MFCC), which is done after preprocessing voice signals. It is then analyzed by CNN and LSTM [16]. Fig. 8 shows a detailed schematic of our proposed process.

*F. Application for Wheelchairs*

The CNN is applied in a wheelchair after the offline training and testing are completed. It aims to perform better accuracy. Then, the next process is to save the CNN model and then embed it into the raspberry pi. There is only a raspberry pi model produced from the CNN model built. As a result, it is not heavy, and the dataset does not need to be embedded in raspberries. Data on the raspberry pi is digital data for moving wheelchairs according to user orders, where data is sent to the motor driver to drive the motor in a wheelchair. The next step is to design a wheelchair and its supporting devices. Fig. 9 shows the hardware and electrical design of a wheelchair.

III. RESULTS AND DISCUSSION

This study discusses the control of a wheelchair using CNN-LSTM as a new control method through its combination offered. There are five types of wheelchair commands: forward, backward, right, left, and stop. Each voice command is taken as many as 1000 data. As a result, total data of 5000 data were acquired and then divided into training data of 4000 and testing data of 1000. For determining the proposed method's performance, two tests of CNN and CNN-LSTM were carried out. Initial testing used CNN with input shape (180.1) and 50 epochs.

Fig. 10. Accuracy using the CNN method

Fig. 10 shows the accuracy level using CNN. The training stage yielded an accuracy of 98.95%, while the testing stage obtained an accuracy of 92.00%. Each processed voice command had a different level of accuracy, as shown in Table II. It occurred because the signal pattern recognition process on each label was different.

The results will be displayed in the form of a confusion matrix to describe the classification model's performance. The following is Fig. 11, which describes the confusion matrix of using CNN. The next test is the combination of CNN-LSTM. By using the same input shape and epoch, here are the test results. This test aims to obtain a better level of accuracy for speech recognition. Fig. 12 shows a graph of the accuracy level using CNN-LSTM.

TABLE II. THE VOICE COMMAND RECOGNITION PROCESS USING THE CNN METHOD

| ***Commands*** | ***Precision*** | ***Recall*** | ***F1-Score*** | ***Support*** |
| --- | --- | --- | --- | --- |
| Forward | 1.00 | 1.00 | 1.00 | 186 |
| Backward | 1.00 | 1.00 | 1.00 | 223 |
| Right | 1.00 | 0.62 | 0.76 | 210 |
| Left | 1.00 | 1.00 | 1.00 | 194 |
| Stop | 0.70 | 1.00 | 0.82 | 187 |
|  | | | | |
| Accuracy | - | - | 0.92 | 1000 |
| Macro  Average | 0.94 | 0.92 | 0.92 | 1000 |
| Weighted  Average | 0.94 | 0.92 | 0.92 | 1000 |



Fig. 11. Confusion matrix voice command recognition with CNN

2020 4th International Conference on Informatics and Computational Sciences (ICICoS) Digital Repository Universitas Jember

recognize voice commands given by users with an accuracy 

rate of 97.80%. This result is influenced by the model of

CNN-LSTM built. The accuracy for each method is different

because of the structure and parameters in the model, such as

learning rate, activation, and dropout. Eventually, this sound

based wheelchair can help the disabled to move more easily

without wasting much energy.

ACKNOWLEDGMENT

Fig. 12. The level of accuracy uses the CNN-LSTM method

TABLE III. THE VOICE COMMAND RECOGNITION PROCESS USES THE CNN METHOD 

| ***Commands*** | ***Precision*** | ***Recall*** | ***F1-Score*** | ***Support*** |
| --- | --- | --- | --- | --- |
| Forward | 1.00 | 1.00 | 1.00 | 186 |
| Backward | 1.00 | 1.00 | 1.00 | 223 |
| Right | 1.00 | 0.90 | 0.94 | 210 |
| Left | 1.00 | 1.00 | 1.00 | 194 |
| Stop | 0.89 | 1.00 | 0.94 | 187 |
|  | | | | |
| Accuracy | - | - | 0.98 | 1000 |
| Macro  Average | 0.98 | 0.98 | 0.98 | 1000 |
| Weighted  Average | 0.98 | 0.98 | 0.98 | 1000 |



Fig. 13. Confusion matrix voice command recognition with CNN-LSTM

The comparison accuracy of both methods is not too significant. The CNN obtained an accuracy of 98.95% with validation accuracy of 92%. However, the combination methods of CNN-LSTM resulted in slightly higher accuracy of 99.15% with validation accuracy of 97.80%. The results of the test process on each voice command and its accuracy are shown in Table III. With a good level of accuracy above, voice commands using CNN-LSTM applied to wheelchairs were intended to get high performance. Nevertheless, there were still voice commands that experienced errors in label recognition, as shown in Fig. 13 below. According to Fig. 13 above, there are no changes that are much different either by using CNN or CNN-LSTM for voice commands of forward, backward, left, right, and stop. Here the error is the voice command Right. If using CNN, this command reads 88 as a stop command. Meanwhile, the CNN-LSTM was less than 22.

CONCLUSION

The application of voice commands to an electric wheelchair using the CNN-LSTM method has a better accuracy level, instead of using CNN. This method can

We want to thank the lecturers and friends, especially at the master's program of electrical engineering, University of Jember, who participated in writing this article to complete it on time.

REFERENCES

[1] M. B. Santoso and N. C. Apsari, “Pergeseran paradigma dalam disabilitas,” vol. 1, no. 2, pp. 166–176, 2017, doi: 10.24198/intermestic.v1n2.6.

[2] C. Joseph, S. Aswin, and J. Sanjeev Prasad, “Voice and gesture controlled wheelchair,” Proc. 3rd Int. Conf. Comput. Methodol. Commun. ICCMC 2019, no. Iccmc, pp. 29–34, 2019, doi: 10.1109/ICCMC.2019.8819662.

[3] P. Arie, “Inklusi Penyandang Disabilitas di Indonesia,” J. Refleks. Huk., vol. 1, pp. 1–4, 2017.

[4] K. P. Tiwari and K. K. Dewangan, “Voice Controlled Autonomous Wheelchair,” Int. J. Sci. Res., no. April, pp. 10–11, 2015.

[5] M. H. Jabardi, “Voice Controlled Smart Electric-Powered Wheelchair Based on Artificial Neural Network Network,” Int. J. Adv. Res. Comput. Sci., vol. 8, no. 5, pp. 31–37, 2017.

[6] M. M. Abdulghani, K. M. Al-Aubidy, M. M. Ali, and Q. J. Hamarsheh, “Wheelchair Neuro Fuzzy Control and Tracking System Based on Voice Recognition,” Sensors (Basel)., vol. 20, no. 10, 2020, doi: 10.3390/s20102872.

[7] P. C A, N. Vijay, and P. Bisen, “Voice Controlled Wheelchair for Physically Disabled People,” Int. J. Res. Appl. Sci. Eng. Technol., vol. 6, no. 5, pp. 2375–2380, 2018, doi: 10.22214/ijraset.2018.5389.

[8] C. N. Anagnostopoulos, T. Iliou, and I. Giannoukos, “Features and classifiers for emotion recognition from speech: a survey from 2000 to 2011,” Artif. Intell. Rev., vol. 43, no. 2, pp. 155–177, 2012, doi: 10.1007/s10462-012-9368-5.

[9] L. Beth, “Mel-Frequency Cepstral Coefficients For Music Modeling,” Cambridge Res. Lab., no. c, pp. 2–6.

[10] A. Elbir, H. O. Ilhan, G. Serbes, and N. Aydin, “Short Time Fourier Transform based music genre classification,” 2018 Electr. Electron. Comput. Sci. Biomed. Eng. Meet. EBBT 2018, pp. 1–4, 2018, doi: 10.1109/EBBT.2018.8391437.

[11] N. Dave, “Feature Extraction Methods LPC , PLP and MFCC In Speech Recognition,” Int. J. Adv. Res. Eng. Technol., vol. 1, no. Vi, pp. 1–5, 2013.

[12] H. S. Kumbhar and S. U. Bhandari, “Speech emotion recognition using MFCC features and LSTM network,” Proc. - 2019 5th Int. Conf. Comput. Commun. Control Autom. ICCUBEA 2019, pp. 2019–2021, 2019, doi: 10.1109/ICCUBEA47591.2019.9129067.

[13] Prabhu, “Understanding of Convolutional Neural Network (CNN) — Deep Learning,” 2018. [Online]. Available: https://medium.com/@RaghavPrabhu/understanding-of

convolutional-neural-network-cnn-deep-learning-99760835f148. [14] Suyanto, K. Nur Ramadhani, and S. Mandala, DEEP LEARNING : Modernisasi Machine Learning Untuk Big Data. Bandung: Informatika Bandung, 2019.

[15] M. Hajiaghayi and E. Vahedi, “Code failure prediction and pattern extraction using LSTM networks,” Proc. - 5th IEEE Int. Conf. Big Data Serv. Appl. BigDataService 2019, Work. Big Data Water Resour. Environ. Hydraul. Eng. Work. Medical, Heal. Using Big Data Technol., no. c, pp. 55–62, 2019, doi: 10.1109/BigDataService.2019.00014.

[16] W. Lim, D. Jang, and T. Lee, “Speech Emotion Recognition using Convolutional and Recurrent Neural Networks,” 2016 Asia-Pacific Signal Inf. Process. Assoc. Annu. Summit Conf., 2017, doi: 10.1109/APSIPA.2016.7820699.